//Please follow these rules to modify register info:
//1. Each comment a line, start with "//", do not append comments at the end
//2. reg block starts and ends with "##"
//3. Each field is composed of [r][reg addr][];[w][reg addr][reg operation][reg value]... 
//4. reg addr and reg value are in terms of hex data, the read reg values will be saved to the third [] in '[r][reg addr][]'
//5. for reg operation, it supports "|", "&" and "A"
//6. for reg read, each reg is supposed to be read with 4 bytes.
//10. "-----------" is meaningless, just to separate the block, clear to see

##[r][0x37100000][];[r][0x37100004][];[w][0x34000014][|][0x];##

