Please reset the STB!
Got sync byte!
Start sending client...
Start to check serial...

Inform slave OK!
Prepare to download...
Start downloading data...
End downloading!
Slave respose OK!
Verify burning flash...
Start burning flash, DONOT POWOFF!

Burning flash OK!


Current UPG exit+++++++!
Current UPG exit--------!FbOTA
save p1 6292152, p2 8388360, p3 6321148
mem start 0x68a48
is_force_key_press hkey 11 , code ffff 
OTA check 0
restore p1 6292152, p2 8388360, p3 6321148
bss_end[0x153838]

 1. stk_ptr[5234688]

MaincodeTaskStart

 2. mem_start[0x153838]

 3. defined MEMORY_END[0x800000]

 4. heap size[6997960]

 5. max syspartition size[2191304]
create patition ok!
init mem ok!
Enable irq!
create timer task ok!
start ap init!
!!!!!!!!!reg_val = 10101010
!!!!!!!!!reg_val = d0d0d10
Hal value 3000108
Hal value 3000108
ts2022
disp_magic_attach
disp magic attach ok!
gpe_soft_attach
!!!!!!CHIP VER: 0x8023
!!!!!!CHIP VER: 0x8023
In driver attach
5840driver_init_time = 410 ms
dm set cache
dm set cache is done
mem_show ---1
mem_show ---2
Partition id: 1
              current free: 1855936
                  max free: 1855936
                      used: 355904
load default start...

lzma:mem[0x23d59c] size[65536]

lzma:malloc [31960]
load default finish.
g_status.crypto_key[i].reserved[2] = 3328
g_status.crypto_key[i].reserved[2] = 3328
g_status.crypto_key[i].reserved[2] = 3328
g_status.crypto_key[i].reserved[2] = 3328
g_status.crypto_key[i].reserved[2] = 3328
g_status.crypto_key[i].reserved[2] = 3328
g_status.crypto_key[i].reserved[2] = 3328
g_status.crypto_key[i].reserved[2] = 3328
g_status.crypto_key[i].reserved[2] = 3328
g_status.crypto_key[i].reserved[2] = 3328
g_status.crypto_key[i].reserved[2] = 3328
g_status.crypto_key[i].reserved[2] = 3328
g_status.crypto_key[i].reserved[2] = 3328
g_status.crypto_key[i].reserved[2] = 3328
g_status.crypto_key[i].reserved[2] = 3328
g_status.crypto_key[i].reserved[2] = 3328
g_status.crypto_key[i].reserved[2] = 3328
g_status.crypto_key[i].reserved[2] = 3328
g_status.crypto_key[i].reserved[2] = 3328
g_status.crypto_key[i].reserved[2] = 3328
g_status.crypto_key[i].reserved[2] = 3328
g_status.crypto_key[i].reserved[2] = 3328
g_status.crypto_key[i].reserved[2] = 3328
g_status.crypto_key[i].reserved[2] = 3328
g_status.crypto_key[i].reserved[2] = 3328
get ver 0

----------------------------------------
 Software version is 
----------------------------------------

mdl_init_time = 600 ms

 RESET FROM SOFTWARE
mtos_task_suspend prio 24
mtos_task_suspend prio 23
mtos_task_suspend prio 30
mtos_task_suspend prio 29
mtos_task_suspend prio 27
mtos_task_suspend prio 28
mtos_task_suspend prio 32
mtos_task_suspend prio 31
mtos_task_suspend prio 26
mtos_task_suspend prio 22
mtos_task_suspend prio 25
mtos_task_suspend prio 10
ui_init_time = 10 ms
ap init ok!
GUI partation is ok
rsc_init is ok
FROM SS: palette id = 0x1
pre gdi_init is ok
REGION:set palette waiting ISR finish!!!
gdi_init is ok
set global alpha = 255
ctrl_init_lib is ok
all classes is ok
[Borden] _switch_playstatus :from_id 0, to_id 1
[Borden] _switch_playstatus : new_ps  1
[Borden] _switch_playstatus : state 1  
switch_autoclose: from 0 to 1 
mtos_task_resume prio 10
mtos_task_resume prio 23
mtos_task_resume prio 24
mtos_task_resume prio 26
UI: active playback.........
mtos_task_resume prio 25
mtos_task_resume prio 22

ACTIVATE EPG
mtos_task_resume prio 30
mtos_task_resume prio 29
enable check lnb[1]
TWIN_PORT_CMD_TURN_OFF
UI: disable vbi insert.........
[borden] ui show logo start--block_id 151, addr 80da072, size 7fd9
p_dev = 16405c, p_vdec = 1640a4
[borden] ui show logo end---
[Borden] _switch_playstatus :from_id 0, to_id 2
[Borden] _switch_playstatus : new_ps  3
UI: switch to LOGO..........
[Borden] _switch_playstatus : PS_LOGO ---> PS_PLAY
stop type[1] sync[1]
##########do_stop 0x0 0x1##

[0x38000004] = 0xc05623cf
---------->>avc av stop
PB stop by sync ticks 380
Before ui_set_subt_display
After ui_set_subt_display
Leave ui_enable_subt
UI: disable ttx.........
[Borden] _switch_playstatus : PS_LOGO ---> PS_PLAY ---> ui_show_logo
[borden] ui show logo start--block_id 148, addr 80d1d74, size 3fee
p_dev = 16405c, p_vdec = 1640a4
[borden] ui show logo end---
switch_autoclose: from 0 to 2 
desktop time update:  2013-1-1, 00:00:02
AP EPG start 4fe000
block size 80000
>>>>>>VBI_CMD_STOP_TTX!!!
TKGS DEBUG : function  tkgs_process_msg_idle, line 146content 327682
channel id 0x0000  filter num 1
channel id 0x0101  filter num 1
channel id 0x0102  filter num 2
channel id 0x0103  filter num 3
update signal
clear_signal_strid 
clear_signal_strid 
